Regarding:  http://forum.openvz.org/index.php?t=tree&goto=27398&#msg_27398

DMESG Output

ovz:~# dmesg
Linux version 2.6.18-openvz-12-1-686 () (ola@concrete) (gcc version 4.1.2 20061115 (prerelease) (Debian 4.1.1-21)) #1 SMP Tue May 1 04:59:12 CEST 2007
BIOS-provided physical RAM map:
 BIOS-e820: 0000000000000000 - 000000000009f800 (usable)
 BIOS-e820: 000000000009f800 - 00000000000a0000 (reserved)
 BIOS-e820: 00000000000ca000 - 00000000000cc000 (reserved)
 BIOS-e820: 00000000000dc000 - 0000000000100000 (reserved)
 BIOS-e820: 0000000000100000 - 000000007cef0000 (usable)
 BIOS-e820: 000000007cef0000 - 000000007ceff000 (ACPI data)
 BIOS-e820: 000000007ceff000 - 000000007cf00000 (ACPI NVS)
 BIOS-e820: 000000007cf00000 - 000000007d000000 (usable)
 BIOS-e820: 00000000fec00000 - 00000000fec10000 (reserved)
 BIOS-e820: 00000000fee00000 - 00000000fee01000 (reserved)
 BIOS-e820: 00000000fffe0000 - 0000000100000000 (reserved)
1104MB HIGHMEM available.
896MB LOWMEM available.
found SMP MP-table at 000f6ce0
On node 0 totalpages: 512000
  DMA zone: 4096 pages, LIFO batch:0
  Normal zone: 225280 pages, LIFO batch:31
  HighMem zone: 282624 pages, LIFO batch:31
DMI present.
ACPI: RSDP (v000 PTLTD                                 ) @ 0x000f6c70
ACPI: RSDT (v001 PTLTD    RSDT   0x06040000  LTP 0x00000000) @ 0x7cefab74
ACPI: FADT (v001 INTEL  440BX    0x06040000 PTL  0x000f4240) @ 0x7cefef14
ACPI: MADT (v001 PTLTD           APIC   0x06040000  LTP 0x00000000) @ 0x7cefef88
ACPI: BOOT (v001 PTLTD  $SBFTBL$ 0x06040000  LTP 0x00000001) @ 0x7cefefd8
ACPI: DSDT (v001 PTLTD  Custom   0x06040000 MSFT 0x0100000d) @ 0x00000000
ACPI: PM-Timer IO Port: 0x1008
ACPI: Local APIC address 0xfee00000
ACPI: LAPIC (acpi_id[0x00] lapic_id[0x00] enabled)
Processor #0 15:2 APIC version 17
ACPI: LAPIC_NMI (acpi_id[0x00] high edge lint[0x1])
ACPI: IOAPIC (id[0x01] address[0xfec00000] gsi_base[0])
IOAPIC[0]: apic_id 1, version 17, address 0xfec00000, GSI 0-23
ACPI: INT_SRC_OVR (bus 0 bus_irq 0 global_irq 2 high edge)
ACPI: IRQ0 used by override.
ACPI: IRQ2 used by override.
ACPI: IRQ9 used by override.
Enabling APIC mode:  Flat.  Using 1 I/O APICs
Using ACPI (MADT) for SMP configuration information
Allocating PCI resources starting at 80000000 (gap: 7d000000:81c00000)
Detected 2398.840 MHz processor.
Built 1 zonelists.  Total pages: 512000
Kernel command line: root=/dev/sda6 ro 
mapped APIC to ffffd000 (fee00000)
mapped IOAPIC to ffffc000 (fec00000)
Enabling fast FPU save and restore... done.
Enabling unmasked SIMD FPU exception support... done.
Initializing CPU#0
PID hash table entries: 4096 (order: 12, 16384 bytes)
Console: colour VGA+ 80x25
Dentry cache hash table entries: 131072 (order: 7, 524288 bytes)
Inode-cache hash table entries: 65536 (order: 6, 262144 bytes)
Memory: 2020820k/2048000k available (1537k kernel code, 25904k reserved, 580k data, 200k init, 1130432k highmem)
Checking if this processor honours the WP bit even in supervisor mode... Ok.
calibrate_delay_direct() failed to get a good estimate for loops_per_jiffy.
Probably due to long platform interrupts. Consider using "lpj=" boot option.
Calibrating delay loop... 1409.02 BogoMIPS (lpj=2818048)
Mount-cache hash table entries: 512
CPU: After generic identify, caps: 0febfbff 00000000 00000000 00000000 00000000 00000000 00000000
CPU: After vendor identify, caps: 0febfbff 00000000 00000000 00000000 00000000 00000000 00000000
CPU: Trace cache: 12K uops, L1 D cache: 8K
CPU: L2 cache: 512K
CPU: After all inits, caps: 0febfbff 00000000 00000000 00000080 00000000 00000000 00000000
Intel machine check architecture supported.
Intel machine check reporting enabled on CPU#0.
Compat vDSO mapped to ffffe000.
Checking 'hlt' instruction... OK.
SMP alternatives: switching to UP code
Freeing SMP alternatives: 16k freed
ACPI: Core revision 20060707
Page beancounter hash is 131072 entries.
CPU0: Intel(R) Pentium(R) 4 CPU 2.40GHz stepping 08
Total of 1 processors activated (1409.02 BogoMIPS).
ENABLING IO-APIC IRQs
..TIMER: vector=0x31 apic1=0 pin1=2 apic2=-1 pin2=-1
Brought up 1 CPUs
migration_cost=0
checking if image is initramfs... it is
Freeing initrd memory: 4383k freed
NET: Registered protocol family 16
ACPI: bus type pci registered
PCI: PCI BIOS revision 2.10 entry at 0xfd9a0, last bus=1
PCI: Using configuration type 1
Setting up standard PCI resources
ACPI: Interpreter enabled
ACPI: Using IOAPIC for interrupt routing
ACPI: PCI Root Bridge [PCI0] (0000:00)
PCI: Probing PCI hardware (bus 00)
PCI quirk: region 1000-103f claimed by PIIX4 ACPI
PCI quirk: region 1040-104f claimed by PIIX4 SMB
Boot video device is 0000:00:0f.0
ACPI: PCI Interrupt Routing Table [\_SB_.PCI0._PRT]
ACPI: PCI Interrupt Link [LNKA] (IRQs 3 4 5 6 7 9 10 11 14 15) *0, disabled.
ACPI: PCI Interrupt Link [LNKB] (IRQs 3 4 5 6 7 *9 10 11 14 15)
ACPI: PCI Interrupt Link [LNKC] (IRQs 3 4 5 6 7 9 10 *11 14 15)
ACPI: PCI Interrupt Link [LNKD] (IRQs 3 4 5 6 7 9 10 11 14 15) *0, disabled.
Linux Plug and Play Support v0.97 (c) Adam Belay
pnp: PnP ACPI init
pnp: PnP ACPI: found 12 devices
PnPBIOS: Disabled by ACPI PNP
PCI: Using ACPI for IRQ routing
PCI: If a device doesn't work, try "pci=routeirq".  If it helps, post a report
PCI: Bridge: 0000:00:01.0
  IO window: disabled.
  MEM window: disabled.
  PREFETCH window: disabled.
PCI: Setting latency timer of device 0000:00:01.0 to 64
NET: Registered protocol family 2
IP route cache hash table entries: 32768 (order: 5, 131072 bytes)
TCP established hash table entries: 131072 (order: 8, 1048576 bytes)
TCP bind hash table entries: 65536 (order: 7, 524288 bytes)
TCP: Hash tables configured (established 131072 bind 65536)
TCP reno registered
Simple Boot Flag at 0x36 set to 0x1
audit: initializing netlink socket (disabled)
audit(1203060858.424:1): initialized
highmem bounce pool size: 64 pages
VFS: Disk quotas dquot_6.5.1
Dquot-cache hash table entries: 1024 (order 0, 4096 bytes)
Initializing Cryptographic API
io scheduler noop registered
io scheduler anticipatory registered
io scheduler deadline registered
io scheduler cfq registered (default)
Limiting direct PCI/PCI transfers.
isapnp: Scanning for PnP cards...
isapnp: No Plug & Play device found
Serial: 8250/16550 driver $Revision: 1.90 $ 4 ports, IRQ sharing enabled
serial8250: ttyS0 at I/O 0x3f8 (irq = 4) is a 16550A
serial8250: ttyS1 at I/O 0x2f8 (irq = 3) is a 16550A
00:09: ttyS0 at I/O 0x3f8 (irq = 4) is a 16550A
00:0a: ttyS1 at I/O 0x2f8 (irq = 3) is a 16550A
RAMDISK driver initialized: 16 RAM disks of 8192K size 1024 blocksize
PNP: PS/2 Controller [PNP0303:KBC,PNP0f13:MOUS] at 0x60,0x64 irq 1,12
serio: i8042 AUX port at 0x60,0x64 irq 12
serio: i8042 KBD port at 0x60,0x64 irq 1
mice: PS/2 mouse device common for all mice
TCP bic registered
NET: Registered protocol family 1
NET: Registered protocol family 17
NET: Registered protocol family 8
NET: Registered protocol family 20
Testing NMI watchdog ... CPU#0: NMI appears to be stuck (1578->1581)!
Using IPI Shortcut mode
Freeing unused kernel memory: 200k freed
Time: tsc clocksource has been installed.
input: AT Translated Set 2 keyboard as /class/input/input0
ACPI: Processor [CPU0] (supports 8 throttling states)
ACPI: Getting cpuindex for acpiid 0x1
ACPI: Getting cpuindex for acpiid 0x2
ACPI: Getting cpuindex for acpiid 0x3
Uniform Multi-Platform E-IDE driver Revision: 7.00alpha2
ide: Assuming 33MHz system bus speed for PIO modes; override with idebus=xx
PIIX4: IDE controller at PCI slot 0000:00:07.1
PIIX4: chipset revision 1
PIIX4: not 100% native mode: will probe irqs later
    ide1: BM-DMA at 0x1058-0x105f, BIOS settings: hdc:DMA, hdd:pio
Probing IDE interface ide1...
pcnet32.c:v1.32 18.Mar.2006 tsbogend@alpha.franken.de
SCSI subsystem initialized
Fusion MPT base driver 3.04.01
Copyright (c) 1999-2005 LSI Logic Corporation
Fusion MPT SPI Host driver 3.04.01
hdc: VMware Virtual IDE CDROM Drive, ATAPI CD/DVD-ROM drive
ide1 at 0x170-0x177,0x376 on irq 15
ACPI: PCI Interrupt 0000:00:11.0[A] -> GSI 18 (level, low) -> IRQ 169
pcnet32: PCnet/PCI II 79C970A at 0x1400, 00 0c 29 06 3c c6 assigned IRQ 169.
eth0: registered as PCnet/PCI II 79C970A
pcnet32: 1 cards_found.
ACPI: PCI Interrupt 0000:00:10.0[A] -> GSI 17 (level, low) -> IRQ 177
mptbase: Initiating ioc0 bringup
ioc0: 53C1030: Capabilities={Initiator}
scsi0 : ioc0: LSI53C1030, FwRev=00000000h, Ports=1, MaxQ=128, IRQ=177
  Vendor: VMware,   Model: VMware Virtual S  Rev: 1.0 
  Type:   Direct-Access                      ANSI SCSI revision: 02
 target0:0:0: Beginning Domain Validation
 target0:0:0: Domain Validation skipping write tests
 target0:0:0: Ending Domain Validation
 target0:0:0: FAST-160 WIDE SCSI 320.0 MB/s DT IU RDSTRM RTI WRFLOW PCOMP (6.25 ns, offset 127)
hdc: ATAPI 1X CD-ROM drive, 32kB Cache, UDMA(33)
Uniform CD-ROM driver Revision: 3.20
SCSI device sda: 209715200 512-byte hdwr sectors (107374 MB)
sda: Write Protect is off
sda: Mode Sense: 5d 00 00 00
sda: cache data unavailable
sda: assuming drive cache: write through
SCSI device sda: 209715200 512-byte hdwr sectors (107374 MB)
sda: Write Protect is off
sda: Mode Sense: 5d 00 00 00
sda: cache data unavailable
sda: assuming drive cache: write through
 sda: sda1 sda2 < sda5 sda6 sda7 sda8 >
sd 0:0:0:0: Attached scsi disk sda
Attempting manual resume
kjournald starting.  Commit interval 5 seconds
EXT3-fs: mounted filesystem with ordered data mode.
pci_hotplug: PCI Hot Plug PCI Core version: 0.5
shpchp: Standard Hot Plug PCI Controller Driver version: 0.4
Linux agpgart interface v0.101 (c) Dave Jones
agpgart: Detected an Intel 440BX Chipset.
agpgart: AGP aperture is 64M @ 0xe8000000
piix4_smbus 0000:00:07.3: Found 0000:00:07.3 device
piix4_smbus 0000:00:07.3: Host SMBus controller not enabled!
input: PC Speaker as /class/input/input1
Real Time Clock Driver v1.12ac
input: ImPS/2 Generic Wheel Mouse as /class/input/input2
parport: PnPBIOS parport detected.
parport0: PC-style at 0x378, irq 7 [PCSPP,TRISTATE]
Floppy drive(s): fd0 is 1.44M
FDC 0 is a post-1991 82077
ts: Compaq touchscreen protocol output
Adding 3903752k swap on /dev/sda5.  Priority:-1 extents:1 across:3903752k
EXT3 FS on sda6, internal journal
loop: loaded (max 8 devices)
device-mapper: ioctl: 4.7.0-ioctl (2006-06-24) initialised: dm-devel@redhat.com
kjournald starting.  Commit interval 5 seconds
EXT3 FS on sda1, internal journal
EXT3-fs: mounted filesystem with ordered data mode.
kjournald starting.  Commit interval 5 seconds
EXT3 FS on sda7, internal journal
EXT3-fs: mounted filesystem with ordered data mode.
kjournald starting.  Commit interval 5 seconds
EXT3 FS on sda8, internal journal
EXT3-fs: mounted filesystem with ordered data mode.
eth1: link up
ACPI: AC Adapter [ACAD] (on-line)
ACPI: Power Button (FF) [PWRF]
NET: Registered protocol family 10
lo: Disabled Privacy Extensions
IPv6 over IPv4 tunneling driver
ip_tables: (C) 2000-2006 Netfilter Core Team
Netfilter messages via NETLINK v0.30.
ip_conntrack version 2.4 (8192 buckets, 65536 max) - 228 bytes per conntrack
eth1: no IPv6 routers present
VE: 101: started
VE: 102: started
VE: 105: started
VE: 106: started
lo: Disabled Privacy Extensions
VE: 110: started
lo: Disabled Privacy Extensions
lo: Disabled Privacy Extensions
VE: 114: started
lo: Disabled Privacy Extensions
VE: 200: started
VE: 201: started
lo: Disabled Privacy Extensions
VE: 202: started
lo: Disabled Privacy Extensions
lo: Disabled Privacy Extensions
VE: 203: started
lo: Disabled Privacy Extensions
VE: 204: started
lo: Disabled Privacy Extensions
VE: 205: started
lo: Disabled Privacy Extensions
VE: 300: started
lo: Disabled Privacy Extensions
lo: Disabled Privacy Extensions
lo: Disabled Privacy Extensions

END